TEST GBR runs

**1. Diff Noise**

NoGo Shallow

LS84bandsGBRSub\_rrs.img

ls8noise.lib

Sensorfilter – LS8BGRN

Error f

RASC 0.7-1.3

Hi\_3 subs

Mid-point start

**2. Diff Noise**

No GoShallow

LS84bandsGBRSub\_rrs.img

ls8noise4BDeep.lib

Sensorfilter – LS8BGRN

Error f

RASC 0.7-1.3

Hi\_3 subs

Mid-point start

**3. Diff Noise**

No GoShallow

LS84bandsGBRSub\_rrs.img

ls8noise4B.lib

Sensorfilter – LS8BGRN

Error f

RASC 0.7-1.3

Hi\_3 subs

Mid-point start

**4. Lower Start Point**

No GoShallow

LS84bandsGBRSub\_rrs.img

ls8noise4B.lib

Sensorfilter – LS8BGRN

Error f

RASC 0.7-1.3

Hi\_3 subs

Quarter Start Point

**5. Lower Start Point – Sum to One**

No GoShallow

LS84bandsGBRSub\_rrs.img

ls8noise4B.lib

Sensorfilter – LS8BGRN

Error f

Sum to One

Hi\_3 subs

Quarter Start Point

**6. Lower Start Point – Sum to One - af**

No GoShallow

LS84bandsGBRSub\_rrs.img

ls8noise4B.lib

Sensorfilter – LS8BGRN

Error af

Sum to One

Hi\_3 subs

Quarter Start Point

**7. Lower Start Point – NAP low range - f**

No GoShallow

LS84bandsGBRSub\_rrs.img

ls8noise4B.lib

Sensorfilter – LS8BGRN

Error f

RASC 0.7-1.3

Hi\_3 subs

Quarter Start Point